Aeroworks Technologies TR-3B Stryker II
REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Flight Manual.doc in the TR-3B Aircraft Folder. For standard procedures, see the Checklists tab.

Max Allowable Gross Weight. | 145,200 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VNE - Maximum Operating Speed | 712 KIAS
MMO - Maximum Operating Speed Mach | .97 Mach
Turbulent Air Penetration Speed | 380 KIAS
VLO - Maximum Gear Operating Speed | 280 KIAS
VLE - Maximum Landing Gear Extension Speed | 300 KIAS
VR - Rotation Speed | 135 KIAS
VSO - Stall Speed (landing cfg.) | 91 KIAS
VS1 - Stall Speed (clean) | 109 KIAS
VREF - Landing Approach Speed | 140 KIAS
Max. Speed on one engine | 360 KIAS
VMC - Min. Controllable (Engine Out) | 158 KIAS
V1 - Takeoff Decision Speed | 123 KIAS
V2 - Takeoff Safety Speed | 145 KIAS
VFE - Flap Extension Speed (Max.) | 250 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.